GSIC - Global Service Information Center

# SECOND COAST BRAKE > REASSEMBLY

## for Preparation Click here

1. INSTALL 2ND COAST BRAKE PISTON ROD

1. Check the piston rod length.

   HINT:
     There are 2 different standard lengths for the piston rod.

   Piston rod length:
   Groove Number | Length
   0 | 78.4 mm (3.087 in.)
   1 | 79.9 mm (3.146 in.)

   If the length is not as specified, replace the rod with a new one even if the brake band works normally.

1. Install the washer plate, compression spring and piston to the piston rod.

1. Firmly hold down the piston, then compress the compression spring.

1. Install the E-ring.

2. INSTALL 2ND COAST BRAKE PISTON OIL SEAL RING

1. Coat the oil seal ring with ATF.

1. Spread the ends of the ring to install the oil seal ring to the piston groove. Then squeeze its ends together.

   NOTICE:
     Do not expand the ring ends excessively.