GSIC - Global Service Information Center

### RADIATOR > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. DRAIN ENGINE COOLANT

4. REMOVE RADIATOR GRILLE

5. REMOVE RADIATOR SIDE DEFLECTOR LH

6. REMOVE RADIATOR SIDE DEFLECTOR RH

7. DISCONNECT RADIATOR HOSE INLET

8. DISCONNECT RADIATOR HOSE OUTLET

9. REMOVE FAN SHROUD

10. DISCONNECT NO. 1 OIL COOLER TUBE INLET (for Automatic Transmission)

11. DISCONNECT NO. 1 OIL COOLER TUBE OUTLET (for Automatic Transmission)

12. REMOVE RADIATOR ASSEMBLY