GSIC - Global Service Information Center

# GENERATOR > INSTALLATION

## for Preparation Click here

1. INSTALL GENERATOR ASSEMBLY

1. Install the generator with the 2 bolts.

   Torque:
     43 N*m{ 438 kgf*cm , 32 ft.*lbf }

1. Install the generator wire with the bolt and nut.

   Torque:
     9.8 N*m{ 100 kgf*cm , 87 ft.*lbf }

1. Connect the connector.

2. INSTALL DRIVE BELT

1. Install the drive belt to the pulleys except the drive belt tensioner pulley.

1. Use the hexagon-shaped part indicated by the arrow in the illustration to move the tensioner pulley downward and then install the drive belt to the tensioner pulley.

   NOTICE:
   1. The backside of the drive belt should face the tensioner pulley.
   2. Check that the drive belt is properly set to each pulley.

1. After a new belt has been installed, check that the tensioner indicator mark is within range A shown in the illustration.

3. INSTALL INTAKE AIR CONNECTOR AND AIR CLEANER ASSEMBLY

1. Install the air cleaner and intake air connector assembly with the 4 bolts, and tighten the hose clamp.

   Torque:
     14 N*m{ 143 kgf*cm , 10 ft.*lbf } for air cleaner
     8.0 N*m{ 82 kgf*cm , 71 in.*lbf } for intake air connector
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf } for hose clamp

1. Connect the MAF meter connector and wire harness clamps.

1. Connect the No. 2 ventilation hose.

1. Connect the vacuum hose.

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.