GSIC - Global Service Information Center

# REAR SPEED SENSOR > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.

1. INSTALL REAR SPEED SENSOR LH

1. Install the sensor with the bolt.

   Torque:
     8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

   NOTICE:
     Make sure the sensor tip is clean.

1. Connect the sensor connector.

2. INSTALL REAR WHEEL

Torque:
  152 N*m{ 1,550 kgf*cm , 112 ft.*lbf } for 2WD (steel type)
  121 N*m{ 1,234 kgf*cm , 89 ft.*lbf } for 2WD (aluminum type)
  105 N*m{ 1,071 kgf*cm , 77 ft.*lbf } for 4WD

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

5. CHECK ABS SPEED SENSOR SIGNAL

1. Check the ABS speed sensor signal (Click here).