GSIC - Global Service Information Center

# HOOD > INSTALLATION

## for Preparation Click here

1. INSTALL HOOD SUB-ASSEMBLY LH

1. Install the hood hinge with the 2 bolts.

   Torque:
     13.0 N*m{ 133 kgf*cm , 10 ft.*lbf }

2. INSTALL HOOD HINGE ASSEMBLY RH

1. Install the hood hinge with the 2 bolts.

   Torque:
     13.0 N*m{ 133 kgf*cm , 10 ft.*lbf }

3. INSTALL HOOD SUB-ASSEMBLY

1. Install the hood with the 4bolts.

   Torque:
     13.0 N*m{ 133 kgf*cm , 10 ft.*lbf }

1. Adjust the hood position (Click here).

4. INSTALL WASHER NOZZLE SUB-ASSEMBLY

1. Connect the washer hose.

1. Engage the 2 claws and install the washer nozzle.