GSIC - Global Service Information Center

### METER / GAUGE SYSTEM > Seat Belt Warning Light for Passenger Seat does not Flash

WIRING DIAGRAM

INSPECTION PROCEDURE

INSPECT FUSE (ECU-IG & GAUGE)

CHECK WIRE HARNESS (ACCESSORY METER*1 OR TELL TAIL LIGHT*2 - BATTERY AND GROUND)

INSPECT FRONT SEAT INNER BELT ASSEMBLY (PASSENGER SIDE)

CHECK WIRE HARNESS (FRONT SEAT INNER BELT ASSEMBLY - BODY GROUND)

CHECK WIRE HARNESS (SEAT INNER BELT - ACCESSORY METER*1 OR TELL TAIL LIGHT*2)

INSPECT FRONT SEAT INNER BELT ASSEMBLY (OCCUPANT DETECTION SENSOR)