GSIC - Global Service Information Center

# FRONT AXLE HUB (for 4WD) > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.
3. A bolt without a torque specification is shown in the standard bolt chart (Click here).

1. INSTALL FRONT AXLE HUB OIL SEAL

1. Using a brass bar and hammer, tap in a new oil seal.

   NOTICE:
     Do not damage the spacer.

2. INSTALL FRONT AXLE BEARING ASSEMBLY

1. Using SST and a press, press a new bearing into the axle hub.

   SST
     09649-17010

3. INSTALL FRONT AXLE HUB ASSEMBLY

1. w/ ABS:
   Install the spacer and ABS rotor to the axle hub.

1. w/o ABS:
   Install the 2 spacers to the axle hub.

1. Apply the MP grease to a new O-ring.

1. Install the new O-ring to the axle hub.

1. Install the dust cover and axle hub to the steering knuckle with the 4 bolts.

   Torque:
     80 N*m{ 816 kgf*cm , 59 ft.*lbf }

4. INSTALL FRONT AXLE HUB NUT LH

1. Install the hub nut.

   Torque:
     235 N*m{ 2,396 kgf*cm , 173 ft.*lbf }

1. Install the adjusting cap and a new cotter pin.

   NOTICE:
     If the holes for the cotter pin are not aligned, tighten the nut an additional 60°.

5. INSTALL FRONT AXLE HUB GREASE CAP

6. INSTALL FRONT DISC

7. INSTALL FRONT DISC BRAKE CALIPER ASSEMBLY

1. Install the disc brake caliper with the 2 bolts.

   Torque:
     123 N*m{ 1,254 kgf*cm , 91 ft.*lbf }

1. Install the brake tube bracket to the steering knuckle with the bolt.

   Torque:
     29 N*m{ 296 kgf*cm , 21 ft.*lbf }

1. Using SST, connect the brake tube to the disc brake caliper.

   SST
     09023-00101

   Torque:
     15 N*m{ 155 kgf*cm , 11 ft.*lbf } for use without SST
     14 N*m{ 143 kgf*cm , 10 ft.*lbf } for use with SST

   HINT:
     Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

8. INSTALL FRONT SPEED SENSOR LH

1. Install the speed sensor with the bolt.

   Torque:
     8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

1. Connect the 2 clamps.

1. Install the speed sensor wire harness to the steering knuckle with the bolt.

   Torque:
     13 N*m{ 133 kgf*cm , 10 ft.*lbf }

9. INSTALL FRONT WHEEL

Torque:
  105 N*m{ 1,071 kgf*cm , 77 ft.*lbf }

10. CHECK ABS SPEED SENSOR SIGNAL

1. Check ABS speed sensor signal (Click here).