GSIC - Global Service Information Center

# REAR SEAT ASSEMBLY (for Extra Cab) > REASSEMBLY

## for Preparation Click here

1. INSTALL REAR SEATBACK COVER

NOTICE:

1. Be careful not to damage the cover.
2. When installing the hog rings, avoid wrinkling the cover.

1. Using hog ring pliers, install the seat cushion cover to the seat cushion pad with 20 new hog rings.

2. INSTALL REAR SEAT CUSHION COVER LH

NOTICE:

2. Be careful not to damage the cover.
3. When installing the hog rings, avoid wrinkling the cover.

1. Using hog ring pliers, install the seat cushion cover to the seat cushion pad with 14 new hog rings.

3. INSTALL REAR SEAT CUSHION COVER RH

HINT:

  Use the same procedures described for the LH side.