GSIC - Global Service Information Center

### METER / GAUGE SYSTEM > Seat Belt Warning Light for Driver Seat does not Operate

## for Preparation Click here

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.INSPECT FRONT SEAT INNER BELT ASSEMBLY (DRIVER SIDE)

1. Disconnect the F12 belt connector.

1. Measure the resistance of the belt.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     1 - 2 | Seat belt is unfastened (ON) | Below 1 Ω
     1 - 2 | Seat belt is fastened (OFF) | 1 MΩ or higher

| NG |

REPLACE FRONT SEAT INNER BELT ASSEMBLY (DRIVER SIDE)

OK |

2.CHECK WIRE HARNESS (FRONT SEAT INNER BELT - COMBINATION METER AND BODY GROUND)

1. Disconnect the F12 belt connector.

1. Disconnect the C8 meter connector.

1. Measure the resistance of the wire harness side connectors.

   Standard resistance:

     Tester Connection | Specified Condition
     F12-1 - C8-11 | Below 1 Ω
     F12-2 - Body ground | Below 1 Ω

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

REPLACE COMBINATION METER ASSEMBLY