GSIC - Global Service Information Center

# HAZARD WARNING SWITCH > INSPECTION

## for Preparation Click here

1. INSPECT HAZARD WARNING SWITCH ASSEMBLY

1. Measure the resistance of the switch.

   Standard resistance:
   Tester Connection | Switch Condition | Specified Condition
   2 (E) - 4 (TB) | OFF | 10 kΩ or higher
   2 (E) - 4 (TB) | ON | Below 1 Ω

   If the result is not as specified, replace the switch assembly.

1. Check illumination operation.

   1. Connect the battery's positive (+) lead to terminal 8 and negative (-) lead to terminal 9. Then check that the Bulb illuminates.

      OK:
        Bulb illuminates.
      If the result is not as specified, replace the switch assembly.