GSIC - Global Service Information Center

# COUNTER GEAR AND REVERSE IDLER GEAR > REMOVAL

## for Preparation Click here

HINT:

  COMPONENTS: Click here.

1. REMOVE NO. 2 COUNTER GEAR FRONT BEARING SNAP RING

1. Using a snap ring expander, remove the snap ring from the counter gear.

2. REMOVE COUNTER GEAR FRONT BEARING

1. Using SST and a press, press out the front bearing from the counter gear.

   SST
     09950-00020
     09950-60010 (09951-00220)
     09950-70010 (09951-07100)

3. INSPECT COUNTER GEAR

1. Using a micrometer, measure the outside diameter of the counter gear as shown in the illustration.

   Standard outside diameter:
     29.984 to 30.000 mm (1.1805 to 1.1811 in.)

   Minimum outside diameter:
     29.984 mm (1.1805 in.)
   If the outside diameter is less than the minimum, replace the counter gear with a new one.