GSIC - Global Service Information Center

# REAR SEAT OUTER BELT ASSEMBLY > INSPECTION

## for Preparation Click here

1. INSPECT REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

1. Before installing the ELR, check the ELR.

   1. When the inclination of the retractor is 15° or less, check that the belt can be pulled from the retractor. When the inclination of the retractor is over 45°, check that the belt locks. .
      If operation is not as specified, replace the seat belt.