GSIC - Global Service Information Center

# FLOOR SHIFT ASSEMBLY > REASSEMBLY

## for Preparation Click here

HINT:

  A bolt without a torque specification is shown in the standard bolt chart (Click here).

1. INSTALL SHIFT LOCK CONTROL ECU SUB-ASSEMBLY

1. Install the ECU with the 2 screws.

2. INSTALL SHIFT LEVER SUB-ASSEMBLY

1. Install the shift lever.

1. Install the pin. Then move the clip downward to lock the pin in place.

3. INSTALL SHIFT LOCK RELEASE BUTTON

1. Install the spring and shift lock release button.

   HINT:
     Securely attach the claws.

4. INSTALL SHIFT LEVER SHAFT HOUSING ASSEMBLY

1. Install the shaft housing with the shift lever guide pin and a new shift lever nut.

   HINT:
     Securely attach the nut.

5. INSTALL POSITION INDICATOR HOUSING LOWER

HINT:

  Securely attach the claw.

6. INSTALL INDICATOR LIGHT WIRE SUB-ASSEMBLY

1. Install the bulb to the position indicator housing.

1. Install the indicator light wire.

   HINT:
     Securely attach the 3 clamps.

7. INSTALL POSITION INDICATOR SLIDE COVER

8. INSTALL POSITION INDICATOR HOUSING UPPER

1. Install the position indicator housing to the shift lever shaft housing.

   HINT:
     Securely attach the claws.

9. INSTALL SHIFT LEVER KNOB SUB-ASSEMBLY

1. Install the knob and twist it clockwise to lock it in place.