GSIC - Global Service Information Center

# FLOOR SHIFT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL FLOOR SHIFT ASSEMBLY

1. Install the floor shift with the 4 bolts.

   Torque:
     14 N*m{ 143 kgf*cm , 10 ft.*lbf }

1. Connect the clamp and 2 connectors.

1. Move the shift lever to L.

1. Connect the transmission control cable.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

4. ADJUST SHIFT LEVER POSITION

1. Adjust the shift lever position (Click here).

5. INSPECT SHIFT LEVER POSITION

1. Inspect the shift lever position (Click here).

6. INSTALL CONSOLE BOX ASSEMBLY

1. Install the console box assembly (Click here).

7. INSTALL UPPER CONSOLE PANEL SUB-ASSEMBLY

1. Install the upper console panel sub-assembly (Click here).

8. INSTALL PARKING BRAKE HOLE COVER SUB-ASSEMBLY

1. Install parking brake hole cover sub-assembly (Click here).

9. INSTALL TRANSFER SHIFT LEVER KNOB SUB-ASSEMBLY