GSIC - Global Service Information Center

# FRONT SEAT OUTER BELT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL SHOULDER BELT ANCHORAGE PLATE COVER (for Double Cab)

1. Install the plate cover as shown in the illustration.

   HINT:
     Make sure the plate cover is firmly set into the garnish's claws.

2. INSTALL FRONT SHOULDER BELT ANCHOR ADJUSTER ASSEMBLY (for Extra Cab and Double Cab)

1. Insert the tip of the adjuster to the pillar, and align the adjuster's bolt hole to the pillar's bolt hole.

1. Install the bolt as shown in the illustration.

   Torque:
     42:
     N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Install the quarter or center pillar garnish (Click here Click here).

3. INSTALL FRONT SEAT OUTER BELT ASSY LH

NOTICE:

  Do not disassemble the retractor.

1. w/o Pretensioner single cab and extra cab:
   Align the claws with the seat belt positioning holes and install the ELR of the seat belt with the bolt as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. w/o Pretensioner Double cab:
   Align the claws with the seat belt positioning holes and install the ELR of the seat belt with the bolt as shown in the illustration.

   Torque:
     4.8 N*m{ 49 kgf*cm , 42 in.*lbf }

1. w/ Pretensioner:
   Install the bolt and seat belt.

   Torque:
     4.8 N*m{ 49 kgf*cm , 42 in.*lbf } for bolt A

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf } for bolt B

1. w/ Pretensioner:
   Connect the pretensioner connector as shown in the illustration.

1. Single cab:
   Install the anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Close the cover.

1. Extra cab and double cab:
   Install the anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Install the cap.

1. Single cab:
   Install the quarter trim panel lower. Then install the seat belt floor anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Extra cab:
   Install the quarter inside trim board. Then install the seat belt floor anchor with the bolt.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

1. Double cab:
   Install the anchor of the seat belt with the built-in bolt after installing the center pillar garnish lower.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.