GSIC - Global Service Information Center

### CONDENSER (for TR Series Engine) > REMOVAL

1. DISCHARGE REFRIGERANT FROM REFRIGERATION SYSTEM

2. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

3. REMOVE RADIATOR GRILLE

4. REMOVE FRONT BUMPER COVER

5. REMOVE FRONT BUMPER REINFORCEMENT SUB-ASSEMBLY

6. DISCONNECT NO. 1 COOLER REFRIGERANT DISCHARGE HOSE

7. DISCONNECT AIR CONDITIONING TUBE AND ACCESSORY ASSEMBLY

8. REMOVE HOOD LOCK ASSEMBLY

9. REMOVE RADIATOR SUPPORT SUB-ASSEMBLY UPPER

10. REMOVE COOLER CONDENSER ASSEMBLY