GSIC - Global Service Information Center

### METER / GAUGE SYSTEM > Entire Combination Meter does not Operate

## for Preparation Click here

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.INSPECT FUSE (DCC, DOME, MET)

1. Remove the DCC and DOME fuses from the engine room junction block.

1. Remove the MET fuse from the instrument panel junction block (driver side junction block).

1. Measure the resistance of the fuses.

   Standard resistance:
     Below 1 Ω

| NG |

REPLACE FUSE

OK |

2.CHECK WIRE HARNESS (COMBINATION METER ASSEMBLY - BATTERY AND BODY GROUND)

1. Disconnect the C8 meter connector.

1. Measure the voltage of the wire harness side connector.

   Standard voltage:

     Tester Connection | Condition | Specified Condition
     C8-1 - Body ground | Always | 10 to 14 V
     C8-21 - Body ground | Ignition switch ON | 10 to 14 V
     C8-21 - Body ground | Ignition switch OFF | Below 1 V

1. Measure the resistance of the wire harness side connector.

   Standard resistance:

     Tester Connection | Specified Condition
     C8-22 - Body ground | Below 1 Ω

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

REPLACE COMBINATION METER ASSEMBLY