GSIC - Global Service Information Center

# FRONT AXLE HUB (for 4WD) > ON-VEHICLE INSPECTION

## for Preparation Click here

1. CHECK FRONT AXLE HUB BEARING

1. Remove the front wheel.

1. Remove the front disc brake caliper (Click here).

1. Remove the front disc.

1. Inspect the axle hub backlash.

   1. Using a dial indicator, check the backlash near the center of the axle hub.

      Maximum:
        0.05 mm (0.0020 in.)
      If the backlash is greater than the maximum, replace the bearing.

1. Inspect the axle hub deviation.

   1. Using a dial indicator, check the deviation at the surface of the axle hub.

      Maximum:
        0.05 mm (0.0020 in.)
      If the deviation is greater than the maximum, replace the bearing.