GSIC - Global Service Information Center

### WATER PUMP > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. DRAIN ENGINE COOLANT

4. DISCONNECT RADIATOR HOSE INLET

5. DISCONNECT RADIATOR HOSE OUTLET

6. REMOVE AIR PUMP INLET (for Unleaded Gasoline Specification Vehicle)

7. REMOVE FAN SHROUD

8. REMOVE GENERATOR ASSEMBLY

9. REMOVE OIL LEVEL GAUGE GUIDE

10. REMOVE NO. 1 IDLER PULLEY SUB-ASSEMBLY

11. REMOVE V-RIBBED BELT TENSIONER ASSEMBLY

12. REMOVE WATER PUMP ASSEMBLY