GSIC - Global Service Information Center

# FRONT WASHER MOTOR > ON-VEHICLE INSPECTION

## for Preparation Click here

1. CHECK WINDSHIELD WASHER MOTOR AND PUMP ASSEMBLY

HINT:

  This check should be performed with the windshield washer motor and pump installed to the washer jar.

1. Fill the washer jar with washer fluid.

1. Connect the battery's positive (+) lead to terminal 1 of the washer motor and pump, and the negative (-) lead to terminal 2.

1. Check that washer fluid flows from the washer jar.

   OK:
     Washer fluid flows from washer jar.
   If the result is not as specified, replace the washer motor and pump assembly.