GSIC - Global Service Information Center

# IGNITION COIL > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE V-BANK COVER

1. Remove the 2 nuts and the V-bank cover.

3. REMOVE AIR CLEANER ASSEMBLY

1. Disconnect the vacuum hose.

1. Disconnect the MAF meter connector.

1. Remove the 2 wire harness clamps.

1. Loosen the 2 hose clamps.

1. Remove the 2 bolts and air cleaner.

4. REMOVE IGNITION COIL ASSEMBLY

1. Disconnect the connector.

1. Remove the bolt and ignition coil.