GSIC - Global Service Information Center

# SIDE TURN SIGNAL LIGHT ASSEMBLY > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH sides.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE SIDE TURN SIGNAL LIGHT ASSEMBLY LH

1. Detach the 2 claws and remove the light as shown in the illustration.

1. Disconnect the connector and remove the side turn signal light.

3. REMOVE SIDE TURN SIGNAL LIGHT BULB

1. Turn the bulb/socket unit in the direction indicated by the arrow and pull to remove it.

1. Remove the bulb from the socket.