GSIC - Global Service Information Center

### STEERING KNUCKLE (for 2WD) > INSTALLATION

1. INSTALL FRONT AXLE HUB INNER BEARING

2. INSTALL FRONT AXLE HUB OIL SEAL

3. INSTALL FRONT AXLE HUB SUB-ASSEMBLY LH

4. INSTALL FRONT AXLE HUB NUT AND ABS SPEED SENSOR ROTOR OR SPACER

5. INSTALL KNUCKLE GREASE RETAINER CAP

6. INSTALL FRONT AXLE HUB ASSEMBLY

7. INSTALL FRONT SUSPENSION UPPER ARM ASSEMBLY LH

8. INSTALL FRONT SUSPENSION LOWER ARM ASSEMBLY WITH ATTACHMENT LH

9. INSTALL TIE ROD END SUB-ASSEMBLY

10. INSTALL FRONT DISC

11. INSTALL FRONT DISC BRAKE CALIPER ASSEMBLY LH

12. INSTALL FRONT SPEED SENSOR

13. BLEED AIR FROM BRAKE LINE

14. CHECK FLUID BRAKE LEVEL IN RESERVOIR

15. CHECK FOR BRAKE FLUID LEAKAGE

16. INSTALL FRONT WHEEL