GSIC - Global Service Information Center

### ENGINE COOLANT TEMPERATURE SENSOR > INSTALLATION

1. INSTALL ENGINE COOLANT TEMPERATURE SENSOR

2. INSTALL INTAKE MANIFOLD

3. INSTALL INTAKE AIR SURGE TANK

4. INSTALL THROTTLE BODY

5. INSTALL AIR CLEANER ASSEMBLY

6. CONNECT NO. 2 VENTILATION HOSE

7. INSTALL V-BANK COVER

8. ADD ENGINE COOLANT

9. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

10. CHECK FOR ENGINE COOLANT LEAKS

11. PERFORM INITIALIZATION