GSIC - Global Service Information Center

# CRANKSHAFT POSITION SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL CRANK SHAFT POSITION SENSOR

1. Apply a light coat of engine oil to the O-ring of the sensor.

1. Install the sensor with the bolt.

   Torque:
     8.5 N*m{ 87 kgf*cm , 75 in.*lbf }

1. Install the 3 clips and connect the sensor connector.

2. INSTALL NO. 2 ENGINE UNDER COVER

3. INSTALL NO. 1 ENGINE UNDER COVER

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.