GSIC - Global Service Information Center

# REAR BRAKE (for 2WD) > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.

1. CHECK BRAKE SHOE LINING THICKNESS

1. Remove the hole plug (check), and check the shoe lining thickness through the hole.

   Minimum thickness:
     1.0 mm (0.039 in.)

   HINT:
     If the thickness is less than the minimum, replace the shoe.

2. REMOVE REAR WHEEL

3. DRAIN BRAKE FLUID

NOTICE:

  Wash off brake fluid immediately if it comes in contact with any painted surface.

4. REMOVE REAR BRAKE DRUM SUB-ASSEMBLY

1. Release the parking brake lever, and remove the drum.

   HINT:
     If the drum cannot be removed easily, perform the following procedures.

1. Remove the hole plug (adjust) and insert a screwdriver into the hole on the backing plate, and hold the automatic adjust lever away from the adjuster.

1. Using another screwdriver, compress the brake shoe adjuster by turning the adjusting wheel.