GSIC - Global Service Information Center

### DTC 01-E2 ON / OFF Indication Parameter Error (AUDIO H/U)

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area
01-E2 | Error occurs in ON / OFF control command from master component. | Radio receiver assembly

## INSPECTION PROCEDURE

1.CHECK FOR DTC

1. Delete the DTC.

1. Check for DTCs again.

   OK:
     No DTC is output.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

END