GSIC - Global Service Information Center

### HEADLIGHT ASSEMBLY > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE RADIATOR GRILLE

3. REMOVE FRONT FENDER LINER LH

4. REMOVE ENGINE SIDE COVER SUB-ASSEMBLY LH (for 4WD)

5. REMOVE ENGINE SIDE COVER SUB-ASSEMBLY RH (for 4WD)

6. REMOVE FRONT BUMPER COVER

7. REMOVE HEADLIGHT ASSEMBLY

8. REMOVE HEADLIGHT SOCKET COVER

9. REMOVE NO. 1 HEADLIGHT BULB

10. REMOVE FRONT TURN SIGNAL LIGHT BULB

11. REMOVE CLEARANCE LIGHT BULB