GSIC - Global Service Information Center

# FRONT NO. 2 SPEAKER > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT DOOR LOWER FRAME BRACKET GARNISH LH

1. Using a screwdriver, detach the 2 clips and remove the garnish.

   HINT:
     Tape the screwdriver tip before use.

3. REMOVE FRONT NO. 2 SPEAKER ASSEMBLY

1. Disconnect the connector.

1. Remove the screw and speaker.