GSIC - Global Service Information Center

# GENERATOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE INTAKE AIR CONNECTOR AND AIR CLEANER ASSEMBLY

1. Disconnect the vacuum hose.

1. Disconnect the No. 2 ventilation hose.

1. Disconnect the MAF meter connector and wire harness clamps.

1. Loosen the hose clamp and remove the 4 bolts, air cleaner and intake air connector assembly.

3. REMOVE DRIVE BELT

1. Use the hexagon-shaped part indicated by the arrow in the illustration to move the tensioner pulley downward and decrease the tension in the drive belt. Then remove the drive belt.

   NOTICE:
     When removing the drive belt, do not use the idle pulley's bolt.

   HINT:
     After removing the drive belt, move the tensioner upward to the maximum amount.

4. REMOVE GENERATOR ASSEMBLY

1. Remove the nut, bolt and generator wire.

1. Disconnect the generator connector.

1. Remove the 2 bolts and generator.