GSIC - Global Service Information Center

# CLUTCH PEDAL (for LHD) > INSTALLATION

## for Preparation Click here

1. INSTALL CLUTCH PEDAL ASSEMBLY

1. Install the clutch pedal.

1. Install the bolt and 2 nuts.

   Torque:
     14 N*m{ 143 kgf*cm , 10 ft.*lbf } for nut A
     24 N*m{ 245 kgf*cm , 18 ft.*lbf } for bolt B

2. INSTALL CLUTCH PEDAL RETURN SPRING

1. Install the pin and new clip.

1. w/o Turn over:
   Install the spring.

3. INSTALL COMBINATION METER ASSEMBLY

NOTICE:

  There are 2 types of combination meters. One type has a 40 pin connector and 16 pin connector. The other type only has a 40 pin connector.

1. Connect all connectors.

1. Install the combination meter with the 3 screws <B>.

4. INSTALL INSTRUMENT CLUSTER FINISH PANEL

1. Attach the 2 claws to install the panel.

1. Install the clip.

5. CHECK FLUID LEVEL IN RESERVOIR

1. Check fluid level in reservoir (Click here).