GSIC - Global Service Information Center

# INTAKE AIR TEMPERATURE SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL INTAKE AIR TEMPERATURE SENSOR

1. Install the sensor and connect the sensor connector.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.