GSIC - Global Service Information Center

# 1GR-FE COOLING > TORQUE SPECIFICATIONS

Coolant:

  Pert Tightened | N*m | kgf*cm | ft.*lbf
  Cylinder head block drain cock plug x Cylinder head | 24.5 | 250 | 18
  No. 1 engine under cover x Body | 28 | 286 | 21

Water pump:

  Pert Tightened | N*m | kgf*cm | ft.*lbf
  Water pump assembly x Timing belt cover | 10 mm head | 9.0 | 92 | 80 in.*lbf
  12 mm head | 23 | 235 | 17
  No. 2 idler pulley sub-assembly x Cylinder head | 39 | 398 | 29
  Water inlet housing x Water pump | 9.0 | 92 | 80 in.*lbf
  Fan shroud x Radiator | 5.0 | 51 | 44 in.*lbf
  Fluid coupling fan x water pump assembly | 21 | 214 | 15
  No. 1 engine under cover x Body | 28 | 286 | 21

Thermostat:

  Pert Tightened | N*m | kgf*cm | ft.*lbf
  Water inlet housing with thermostat x Water inlet | 9.0 | 92 | 80 in.*lbf
  No. 1 engine under cover x Body | 28 | 286 | 21

Fan:

  Pert Tightened | N*m | kgf*cm | ft.*lbf
  Fluid coupling x Fan | 6.0 | 61 | 53 in.*lbf

Radiator:

  Pert Tightened | N*m | kgf*cm | kgf*cm
  Radiator assembly x Body panel | 12 | 122 | 9
  Fan shroud x Radiator assembly | 5.0 | 51 | 44 in.*lbf
  Fluid coupling x Water pump assembly | 21 | 214 | 15
  Oil reservoir x Radiator assembly | 5.0 | 51 | 44 in.*lbf
  No. 1 engine under cover x Body | 28 | 286 | 21