GSIC - Global Service Information Center

OIL PUMP > INSPECTION > Preparation |

EQUIPMENT
Drain hose |
Feeler gauge |
Torque wrench |

LUBRICANT
Item | Capacity | Classification
Oil grade | - | API grade SL or SJ, Energy-Conserving or ILSAC, multigrade engine oil
Drain and refill with oil filter change | 5.5 liters (5.8 US qts, 4.8 Imp qts.) | -
Drain and refill without oil filter change | 5.2 liters (5.5 US qts, 4.6 Imp qts.) | -
Dry fill | 6.6 liters (7.0 US qts, 5.8 Imp qts.) | -

SSM
| 08826-00080 | Seal Packing Black or equivalent (FIPG) | -
| 08826-00100 | Seal Packing 1282B, THREE BOND 1282B or equivalent (FIPG) | -
| 08833-00070 | Adhesive 1324, THREE BOND 1324 or equivalent | -