GSIC - Global Service Information Center

INPUT SHAFT > REMOVAL > Preparation |

SST
| 09527-10011 | Rear Axle Shaft Bearing Remover

EQUIPMENT
Cylinder gauge | -
Dial indicator or dial indicator with magnetic base | -
Feeler gauge | -
Micrometer | -
Plastic hammer | -
Press | -
Torque wrench | -
Vernier calipers | -

LUBRICANT
Item | Capacity | Classification
Manual transmission oil | 2.2 liters (2.3 US qts, 1.9 lmp. qts) | API GL-4 or GL-5 SAE 75W-90

RECOMMENDED TOOLS
| 09031-00040 | Pin Punch . | -
| 09042-00020 | Torx Socket T40 | -
| 09905-00012 | Snap Ring No.1 Expander | -

SSM
| 08826-00090 | Seal Packing 1281, THREE BOND 1281 or equivalent (FIPG) | -
| 08833-00080 | Adhesive 1344 THREE BOND 1344 LOCTITE 242 or equivalent | -