GSIC - Global Service Information Center

TIMING BELT > INSPECTION > Preparation |

EQUIPMENT
Abrasive compound | Valve
Brush | Piston
Caliper gauge | -
Carbide cutter (25°) | Valve seat
Carbide cutter (45°) | Valve seat
Carbide cutter (75°) | Valve seat
Connecting rod aligner | -
Cylinder gauge | -
Dial indicator | -
Dye penetrant | -
Groove cleaning tool | Piston ring groove
Heater | -
Magnetic finger | -
Micrometer | -
Pin hole grinder | Connecting rod bush
Piston ring compressor | -
Piston ring expander | -
Plastigage | -
Precision straight edge | -
Press | -
Razor brade | -
Reamer (6.0 mm) | Valve guide bush
Ridge reamer | Cylinder
Soft brush | Cylinder head
Cylinder block
Solvent | -
Spring tester | Valve spring
Steel square | Valve spring
Thermometer | -
Torque wrench | -
Valve seat cutter | -
Valve guide bushing brush | -
V-block | -
Vernier calipers | -
Wire brush | Vale
Cylinder head

RECOMMENDED TOOLS
| 09040-00011 | Hexagon Wrench Set | -
| 09090-04020 | Engine Sling Device | -
| 09200-00010 | Engine Adjust Kit | -

SSM
| 08826-00080 | Seal Packing Black or equivalent (FIPG) | -
| 08833-00070 | Adhesive 1324, THREE BOND 1324 or equivalent | -