GSIC - Global Service Information Center

DIFFERENTIAL VACUUM ACTUATOR > REPLACEMENT > Preparation |

EQUIPMENT
Brass bar | -
Chisel | -
Dial indicator | -
Feeler gauge | -
Hammer | -
Micrometer | -
Needle nose pliers | -
Plastic hammer | -
Press | -
Red lead | -
Screwdriver | -
Tape | -
Torque wrench | -
Vernier calipers | -

LUBRICANT
Item | Capacity | Classification
Front differential | w/ A.D.D. | 1.60 to 1.70 liters (1.69 to 1.80 US qts, 1.40 to 1.50 lmp. qts.) | Hypoid gear oil APL GL-5 Above-18°C (0°F): SAE 90) Below-18°C (0°F): SAE 80W or 80W-90
w/o A.D.D. | 1.40 to 1.50 liters (1.48 to 1.59 US qts, 1.23 to 1.31 lmp. qts.) | Hypoid gear oil APL GL-5 Above-18°C (0°F): SAE 90) Below-18°C (0°F): SAE 80W or 80W-90
Rear differential | 2WD | 3.15 to 3.25 liters (3.30 to 3.43 US qts, 2.77 to 2.86 lmp. qts.) | Hypoid gear oil APL GL-5 Above-18°C (0°F): SAE 90) Below-18°C (0°F): SAE 80W or 80W-90
4WD | 3.30 to 3.40 liters (3.49 to 3.59 US qts, 2.90 to 2.99 lmp. qts.) | Hypoid gear oil APL GL-5 Above-18°C (0°F): SAE 90) Below-18°C (0°F): SAE 80W or 80W-90

RECOMMENDED TOOLS
| 09011-12301 | Socket Wrench 30 mm | -
| 09031-00030 | Pin Punch | -
| 09044-00010 | Torx Socket E14 | -
| 09905-00012 | Snap Ring No.1 Expander | -
| 09905-00013 | Snap Ring Pliers | -

SSM
| 08833-00090 | Adhesive 1131, THREE BOND 1131, LOCTITE 518 or equivalent | -
| 08833-00100 | THREE BOND 1360K or equivalent | -