GSIC - Global Service Information Center

POWER WINDOW CONTROL SYSTEM > Front Passenger Side Power Window does not Operate with Front Passenger Side Power Window Switch > Preparation |

EQUIPMENT
Adhesive | -
Knife | -
Piano wire | -
Plastic sheet | -
Sealer gun | -
Torque wrench | -
Tape | -
Wooden block or similar object | -

RECOMMENDED TOOLS
| 09082-00040 | TOYOTA Electrical Tester |

SSM
| 08850-00801 | Windshield Glass Adhesive Set or equivalent |