GSIC - Global Service Information Center

OIL PUMP > COMPONENTS > Preparation |

EQUIPMENT
Feller gauge |
Torque wrench |

LUBRICANT
Item | Capacity | Classification
Oil grade | - | API grade SL or SJ, Energy-Conserving or ILSAC, multigrade engine oil
Drain and refill with oil filter change | 5.6 liters (5.9 US qts, 4.9 Imp qts.) | -
Drain and refill without oil filter change | 5.3 liters (5.6 US qts, 4.6 Imp qts.) | -
Dry fill | 6.3 liters (6.7 US qts, 5.5 Imp qts.) | -

SSM
| 08826-00080 | Seal Packing Black or equivalent (FIPG) | -