GSIC - Global Service Information Center

RADIATOR > ON-VEHICLE CLEANING > Preparation |

COOLANT
Item | Capacity | Classification

Engine coolant

7.0 liters (7.4 US pts, 6.2 lmp. qts)

Use only "TOYOTA Super Ling Life Coolant (SLLC)" or similar high quality ethylene glycol based non-silicate, non-amine, non-nitrite and non-borate coolant with long-life hybrid organic acid technology (coolant with long-life hybrid organic acid technology consists of a combination of low phosphates and organic acids).

EQUIPMENT
Torque wrench | -
Radiator cap tester | -
Heater | -