GSIC - Global Service Information Center

RADIATOR > REMOVAL > Preparation |

COOLANT
Item | Capacity | Classification

Engine coolant
A/T

11.1 liters (11.7 US pts, 9.8 lmp. qts)

Use only "TOYOTA Super Ling Life Coolant (SLLC)" or similar high quality ethylene glycol based non-silicate, non-amine, non-nitrite and non-borate coolant with long-life hybrid organic acid technology (coolant with long-life hybrid organic acid technology consists of a combination of low phosphates and organic acids).

Engine coolant M/T | 9.8 liters (10.4 US pts, 8.6 lmp. qts)

EQUIPMENT
Torque wrench | -
Radiator cap tester | -
Heater | -