GSIC - Global Service Information Center

ENGINE OIL COOLER > INSPECTION > Preparation |

EQUIPMENT
Oil pressure gauge | -
Radiator cap tester | -
Torque cap tester | -
Vernier caliper | -
Wooden block | -
Precision straightedge | -

LUBRICANT
Item | Capacity | Classification
Oil grade | - | G-DLD1 or API grade CF-4, CF
Drain and refill | with oil filter change | 6.9 liters (7.3 US qts, 6.1 lmp, qts) | -
without oil filter change | 6.6 liters (7.0 US qts, 5.8 lmp, qts) | -
Dry fill | 7.4 liters (7.8 US qts, 6.5 lmp, qts) | -

RECOMMENDED TOOLS
| 09090-04020 | Engine Sling Device | -
| 09200-00010 | Engine Adjust Kit | -

SSM
| 08826-00080 | Seal Packing Black or equivalent (FIPG) | -
| 08833-00070 | Adhesive 1324, THREE BOND 1324 or equivalent | -