1. | A range indicator | 2. | Shift position indicator | 3. | M range indicator
4. | Transmission warning light | 5. | Information display | 6. | Paddle shifter (shift-down switch)
7. | Paddle shifter (shift-up switch) | 8. | Stop lamp switch | 9. | Accelerator pedal position sensor
10. | Set-up switch | 11. | Range sensor | 12. | Auto/Manual range change switch
13. | TCM | 14. | TCM relay | 15. | Back-up lamp relay
16. | Transmission connector | 17. | Output shaft speed sensor | 18. | Clutch A speed sensor
19. | Clutch B speed sensor | 20. | Heat exchanger | 21. | Actuator control module
22. | Fluid temperature sensor | 23. | Front control module | 24. | Park position switch
A. | Combination meter | B. | Steering assembly | C. | Rear of LH instrument lower panel
D. | Center console | E. | Control device assembly | F. | Trunk room
G. | Left side of trunk room | H. | Transmission assembly |  |
The following parts are integrated into the actuator control module (21).
| Axis A feed pressure solenoid valve |  | Axis B feed pressure solenoid valve |  | Shift solenoid valve 1
| Shift solenoid valve 2 |  | Shift solenoid valve 3 |  | Shift solenoid valve 4
| Sequence solenoid valve |  | Line pressure sensor |  | 1st-Reverse position sensor 1
| 1st-Reverse position sensor 1 |  | 2nd-4th position sensor |  | 6th-Neutral position sensor
| 3rd-5th position sensor |  |  |  |
The following parts are integrated into the front control module (23).
| Line pressure solenoid valve |  | Clutch A solenoid valve |  | Clutch B solenoid valve
| Lubricating flow solenoid valve |  | Clutch A pressure sensor |  | Clutch B pressure sensor