REMOVAL ■ CAUTION ■

- Never spill or splash brake fluid on painted surfaces. Brake fluid may seriously damage paint. Wipe it out immediately and wash with water if it gets on a painted surface.
- Wrap the flare nut wrench with waste cloth to protect the caliper from damage.
- If the brake fluid adheres to the caliper or disc rotor, quickly wipe it out.

1.Remove tires with power tool. Refer to Exploded View.

2.Drain brake fluid. Refer to Draining.

3.Loosen the flare nut with a flare nut wrench and separate the brake tube from the hose and caliper.
■ CAUTION ■

- Never scratch the flare nut and the brake tube.
- Never bend sharply, twist or strongly pull out the brake hoses and tubes.
- Cover open end of brake tubes and hoses when disconnecting to prevent entrance of dirt.

4.Remove brake tube mounting bolt.

5.Remove brake hose mounting nut.

6.Remove the lock plate and remove the brake hose.

INSTALLATION
■ CAUTION ■

- Never spill or splash brake fluid on painted surfaces. Brake fluid may seriously damage paint. Wipe it out immediately and wash with water if it gets on a painted surface.
- Wrap the flare nut wrench with waste cloth to protect the caliper from damage.
- If the brake fluid adheres to the caliper or disc rotor, quickly wipe it out.
- Never allow foreign matter (e.g. dust) and oils other than brake fluid to enter the reservoir tank.
- Since brake fluid is susceptible to deterioration from moisture, discard brake fluid remaining in the container.

1.Install the brake tube to the brake hose, temporarily tighten the flare nut by hand until it does not rotate further, and fix the brake hose to the bracket with the lock plate.
■ CAUTION ■
Check that all brake hoses and tubes are not twisted or bent.

2.Install brake hose mounting nut.
■ CAUTION ■
Never reuse brake hose mounting nut.

3.Install brake tube mounting bolt.

4.Tighten the flare nut to the specified torque with a flare nut crowfoot and a torque wrench.
■ CAUTION ■
Never scratch the flare nut and the brake tube.

5.Refill with new brake fluid and perform the air bleeding. Refer to Bleeding Brake System.
■ CAUTION ■
Never reuse drained brake fluid.