REMOVAL

1.Remove main muffler assembly. Refer to Exploded View.

2.Remove rear wheel sensor. Refer to Exploded View (GT-R certified NISSAN dealer).

3.Remove rear drive shaft. Refer to Exploded View (GT-R certified NISSAN dealer).

4.Install attachment (A) to side flange to pull out the side flange with the sliding hammer (B).

A | : Attachment [SST: KV401010000 ( — )]
B | : Sliding hammer [SST: ST36230000 (J-25840‐A)]

NOTE：
After side flange removed, comfirm that circular clip is remaining in side gear of differential assembly.

5.Remove side oil seal.
■ CAUTION ■
Never damage transmission assembly.

INSTALLATION

1.Install side oil seal (gear carrier side) with the drift (A) [SST: KV40104830 ( — )] within the dimension (L) shown as follows.

L | : 6.3 – 7.3 mm (0.248 – 0.287 in)

■ CAUTION ■

- Never reuse oil seal.
- When installing, never incline oil seal.
- Apply multi‐purpose grease to side oil seal lip.

2.Install side oil seal (side cover side) with the drift [SST: KV40104830 ( — )] until the side oil seal becomes flush with the side cover end.
■ CAUTION ■

- Never reuse oil seal.
- When installing, never incline oil seal.
- Apply multi‐purpose grease to side oil seal lip.

3.Install side flange according to the steps.

(1)Attach the protector (A) [SST: KV38105500 (J‐33904)] to side oil seal (2).

(2)Insert side flange (1), and engage the serrated part of the flange with that of the side gear to remove protector.

(3)Put a suitable drift on the center of side flange and drive the drift until sound changes.
NOTE：
Driving sound of the side flange changes to echo‐like sound after complete installation.

(4)Check that the installation measurement (A) of the side flange is as follows.

A | : 370 mm (14.57 in)

4.Install rear drive shaft. Refer to Exploded View (GT-R certified NISSAN dealer).

5.Install rear wheel sensor. Refer to Exploded View (GT-R certified NISSAN dealer).

6.Install main muffler. Refer to Exploded View.

7.When oil leaks while removing, check oil level after the installation. Refer to Inspection.