REMOVAL

1. | Blower unit | 2. | Heater & cooling unit assembly | 3. | Steering member
4. | Instrument panel assembly |  |  |  |
Refer to Components for symbols in the figure.

DISASSEMBLY

1. | Ventilator seal | 2. | Ventilator door | 3. | Defroster seal
4. | Defroster door (right) | 5. | Foot door lever | 6. | Defroster door lever
7. | Foot door link | 8. | Ventilator door spring | 9. | Ventilator door lever
10. | Ventilator door link | 11. | Main link | 12. | Mode door motor bracket
13. | Mode door motor | 14. | Main link sub | 15. | Max. cool door link
16. | Defroster door link | 17. | Max. cool door lever | 18. | Air mix door motor (passenger side)
19. | Air mix door adapter | 20. | O‐ring | 21. | Low‐pressure pipe 1
22. | High‐pressure pipe 3 | 23. | Cooler pipe grommet | 24. | Insulator
25. | Heater pipe grommet | 26. | Heater pipe cover | 27. | Heater duct
28. | Foot duct (left) | 29. | Air mix door motor (driver side) | 30. | Air mix door adapter
31. | Heater & cooling unit case (left) | 32. | Aspirator | 33. | Aspirator hose
34. | Packing | 35. | Packing | 36. | Defroster door (left)
37. | Rear ventilator cover | 38. | Center case | 39. | Heater & cooling unit case (right)
40. | Foot duct (right) | 41. | Drain hose | 42. | Evaporator cover
43. | Expansion valve | 44. | Evaporator | 45. | Evaporator cover adapter
46. | Heater pipe bracket | 47. | Heater core | 48. | Packing
49. | Foot door (right) | 50. | Rear ventilator door | 51. | Foot door (left)
52. | Max. cool door (right) | 53. | Max. cool door (left) | 54. | Air mix door (Slide door)
55. | Intake sensor | 56. | Intake sensor bracket |  |
Refer to Components for symbols in the figure.