DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1130 | ENGINE SIGNAL 1 | Major engine components are malfunctioning. |

- Harness or connector
- ABS actuator and electric unit (control unit)
- ECM
- CAN communication line

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Turn the ignition switch ON.
2. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1130” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END