When doing work that applies to the list below, make sure to adjust neutral position of steering angle sensor before running vehicle.

×: Required –: Not required
Situation | Adjustment of steering angle sensor neutral position
Removing/Installing ABS actuator and electric unit (control unit) | —
Replacing ABS actuator and electric unit (control unit) | ×
Removing/Installing steering angle sensor | ×
Replacing steering angle sensor | ×
Removing/Installing steering components | ×
Replacing steering components | ×
Removing/Installing suspension components | ×
Replacing suspension components | ×
Changing old tires to new ones | —
Adjusting wheel alignment | ×