■ CAUTION ■ Under the following conditions, ABS is activated and vibration is felt when brake pedal is lightly depressed (just place a foot on it). However, this is normal.

- When shifting gears
- When driving on slippery road
- During cornering at high speed
- When passing over bumps or grooves [approximately 50 mm (1.97 in) or more]
- When pulling away just after starting engine [approximately 10 km/h (6 MPH) or higher]

1.SYMPTOM CHECK 1
Check that there is pedal vibration when the engine is started.
Does vibrations occur?
YES>>GO TO 2.
NO>>Inspect the brake pedal.
2.SYMPTOM CHECK 2
Check that there is ABS operation noises when the engine is started.
Does the operation noise occur?
YES>>GO TO 3.
NO>>Perform self-diagnosis for “ABS” with CONSULT-III.
3.SYMPTOM CHECK 3
Check symptoms when electrical component (headlamps, etc.) switches are operated.
Do symptoms occur?
YES>>Check if there is a radio, antenna, antenna lead wire, or wiring close to the control unit. If there is, move it farther away.
NO>>Normal