WORK SUPPORT

Service item | Setting item | Setting
BATTERY SAVER SET | On* | With the exterior lamp battery saver function
Off | Without the exterior lamp battery saver function
ROOM LAMP BAT SAV SET | On* | With the interior room lamp battery saver function
Off | Without the interior room lamp battery saver function
ROOM LAMP TIMER SET | MODE 1* | 30 min. | Sets the interior room lamp battery saver timer operating time.
MODE 2 | 60 min.
*: Factory setting

DATA MONITOR

Monitor item [Unit] | Description
REQ SW-DR [On/Off] | The switch status input from request switch (driver side)
REQ SW-AS [On/Off] | The switch status input from front request switch (passenger side)
REQ SW-RR [On/Off] | NOTE： The item is indicated, but not monitored.
REQ SW-RL [On/Off] | NOTE： The item is indicated, but not monitored.
PUSH SW [On/Off] | The switch status input from push-button ignition switch
ACC RLY-F/B [On/Off] | NOTE： The item is indicated, but not monitored.
KEY SW-SLOT [On/Off] | Key switch status input from key slot
UNLK SEN-DR [On/Off] | Driver door unlock status input from unlock sensor
DOOR SW-DR [On/Off] | The switch status input driver side front door switch
DOOR SW-AS [On/Off] | The switch status input from passenger side door switch
DOOR SW-RR [On/Off] | NOTE： The item is indicated, but not monitored.
DOOR SW- RL [On/Off] | NOTE： The item is indicated, but not monitored.
DOOR SW-BK [On/Off] | NOTE： The item is indicated, but not monitored.
CDL LOCK SW [On/Off] | Lock switch status received from the door lock and unlock switch
CDL UNLOCK SW [On/Off] | Unlock switch status received from the door lock and unlock switch
KEY CYL LK-SW [On/Off] | NOTE： The item is indicated, but not monitored.
KEY CYL UN-SW [On/Off] | NOTE： The item is indicated, but not monitored.
TRNK/HAT MNTR [On/Off] | The switch status input from trunk room lamp switch
RKE-LOCK [On/Off] | Lock signal status received from remote keyless entry receiver
RKE-UNLOCK [On/Off] | Unlock signal status received from remote keyless entry receiver

ACTIVE TEST

Test item | Operation | Description
BATTERY SAVER | Off | Cuts the interior room lamp power supply to turn interior room lamp OFF.
On | Outputs the interior room lamp power supply to turn interior room lamp ON.*
*: Each lamp switch is in ON position.